# Here we created an appropriate =.in with the correct
# lattice. The we used xfplo -fs to setup and export a k-mesh to =.kp.
# We use slabify to calculate the Fermisurface corresponding to the
# model data in ../+hamdata.
#
# run

./slabify.py | tee out
xfplo =.xef

# to see the result.
